PREMIER INSPECTION
$1599

 
PARKEROCEANIC appreciates your business and looks forward to providing you with the most advanced RV inspection available in today’s RV market. So that we may provide you with a thorough inspection, your RV will need to be hooked up to all the utilities -fresh water, electricity and sewer during the inspection. If that is not possible call me.
 
Due to the nature of RV absorption refrigerators and the time it takes for these refrigerators to cool, the refrigerator must have been in operation for at least 12 hours before an accurate temperature reading can be taken in the freezer and the refrigerator compartments.
 
This report will consist of 50 to 100 photos describing the items that have been identified during the detailed Premier Inspection.
 
Roof
Inspect and rate the overall roof condition
Evaluate the condition of the various sealant and joints around the roofing components
Rate the condition of the roof vents, air conditioners, antenna and other components that are mounted on the roof
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Sidewall and End Caps
Inspect and evaluate the appearance and functional condition of the end caps, sidewalls, entrance doors, windows and cargo access doors
Inspect and evaluate any damage, discoloration and delamination of the side wall and end cap components
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Slideout Rooms
Inspect and rate the roof condition
Inspect and evaluate the condition of the seals, sweeps and gaskets for possible damage
Evaluate the attached wiring and utility harness that feed underneath the Slideout room
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Awnings and Slideout Toppers
Operate and rate condition of the awning frames and latching mechanisms
Evaluate and rate the condition of fabric material of the awnings
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Chassis Turn Signal and Running Lights (12 volt DC)
Operate and evaluate the emergency break a away switch
Activate and evaluate the operation of the DOT lights mounted on the RV
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
120 Volt AC Electrical System (house type power)
Inspect and rate the condition of the power cord and its connection ends
Remove cover panel of 120 volt circuit breaker box to visually inspect the condition of the wiring, circuit breakers and grounding connections
Test and verify the output operation of the 120 VAC to 12 VDC converter for charging of the deep cycle batteries
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Generator  if installed *strongly recommend performing oil analysis to determine internal combustion engine component condition.
Identify and note the model, serial number and run hours of the generator
Check oil level
Start, operate and test the onboard generator
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Inverter if installedIdentify and note the model and serial number of the inverter
Visually inspect the wiring and electrical connections and fuses/circuit breakers
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Coach Battery System  (12 volt DC deep cycle Battery Electrical System)
Locate and note the location of the battery stack
Evaluate the condition, age and matched sizing of the battery stack
Access and visually inspect the wiring, fuse panel and fuses of the 12 volt DC electrical system
Evaluate the operation of the fresh water /waste water monitor panel for incorrect tank readings
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Fresh Water System
Verify the fresh water connections for the city water hookup are operational
Verify the onboard fresh water tank and pressure pump system will operate and maintain pressure
Operationally test all fresh water fixtures inside and outside of the RV
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Waste Water Systems  (Gray and Black Water)
Operationally test and inspect both waste (gray and black) plumbing systems for leaks under the sinks, shower, around the toilet and discharge lines
Operate both drain valves and test for ease of operation
Verify the drain cap is in place and will hold waste water
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Life Safety Items
Test the Ground Fault Circuit Interrupter (GFCI) circuits in the 6 foot range of the water areas of the bathroom, kitchen and exterior receptacles
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Test all wall receptacles for correct polarity and ground fault
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Test the exterior skin for hot skin that would cause electrical shock
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Emergency Exit Windows  Verify all safety windows are operational
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Fire Extinguisher  Verify unit is secure in bracket and dial indicates extinguisher is fully charged
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Smoke/Fire Detector Test and verify operation of unit and document expiration date of detector
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Carbon Monoxide Detector (if applicable)  Test and verify operation of unit and document expiration date of detector
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
LP Gas Detector  Verify gas detection and audio alarm. Document expiration date of detector
Verify the rubber grommet is properly sealed around LP gas line of water heater
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
LP Gas System
Visually inspect all hoses and pressure regulators for damage and age deterioration
Verify plastic cover has been installed over regulator
On split tank system verify the red colored single stage regulator is installed
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
DOT Cylinders - if equipped
Document the manufacture date of DOT cylinders
List the tank sizes that have been installed
Conduct visual inspection of exterior of cylinder for rust and other damage
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
ASME tank - if equipped
If tank is visible, conduct a visual inspection of tank for rust or physical damage
Document the manufacture date of the ASME tank if accessible
List the gallon capacity of the tank
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
 
Refrigerator
Identify the brand, model and type of refrigerator
Operate on all heat sources - 120 volt AC, LP gas and for 3 way refrigerators, 12 volt DC
Collect serial and model number and verify with manufacturer if recall notice has been issued and completed for this unit
Test for interior temperature of upper and lower refrigerator compartments and ice maker (if installed) *if refrigerator has been operating for minimum of 12 hours
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
 
Water Heater
Identify the brand, model and type of water heater
Visually inspect burner assembly and gas exhaust system for blockages and insect infestation
Fill tank with water (if necessary) and verify operation on all heat sources  LP gas and 120 volt AC if equipped with heating element
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Furnace
If accessible, identify the brand, model and type of furnace(s) that have been installed
Visually inspect air intake and exhaust assemblies for blockages and insect infestation
Operate and verify warm air discharge out of vents and proper return air flow to unit
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Cooktop/ Stove
Evaluate and rate the condition of the cooktop or stove
Verify the ignition and operation of all top burners and the oven flame (if equipped)
Inspect and rate the condition of the metal grill top and rubber grommets of top burner area
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Air Conditioner(s)
Identify and list the type of cooling unit/heat pump
Perform cooling efficiency test (Delta T) on each unit
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Washer/ Dryer
Visually inspect and verify a wash and rinse cycle of the washer and dryer
Evaluate and rate the exterior condition of the dryer exhaust vent
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Microwave/Convection Oven
Identify and list the brand, model, type and output wattage of the unit
Operate unit for 60 seconds utilizing cup of water and then list water temperature
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Dishwasher - if installed
Identify and list the brand and model of unit
Verify operation of unit and inspect for leaks and non- functioning rotating racks and wash bars.
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
 In House Vacuum System if installed
Identify and list the brand and model of unit
Verify the operation and visually inspect the various components of the hose assembly, access doors and dirt bag
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Electric Fireplace  if installed
Identify and list the brand and model of unit
Operate and verify the various heat settings, fan speed levels and the back lighting
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Cooktop Exhaust Fan
Operate and verify condition of the exhaust function and fan speeds
Evaluate and rate the exterior condition of the exhaust vent
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Ceiling Mounted Fans and Ceiling Exhaust Vents
Visually inspect the condition of the blades and motor
Operate and verify condition of the blade direction and fan speeds
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Interior Conditions and Appearance
Visually inspect all ceilings, walls, interior doors and flooring for signs of water intrusion, surface damage and/or staining
Operate all windows and doors noting any deficiencies or missing components
Operate all interior, exterior and decor lighting - 12 volt and 120 volt
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Cabinets and Closet Condition
Inspect and evaluate all cabinet doors, drawers and pull out operation
Visually inspect all counter tops and flat surface areas of the kitchen, living room, bathroom, bedroom and storage areas for scratches and damage
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Furniture
Visually inspect the condition of the dinette table/booth, chairs, recliners and sofa
Inspect and note furniture fabric tears, discoloration and signs of excessive wear
Visually inspect and note signs of mattress damage or staining
  Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
 Entertainment System
Visually inspect and operate all TV and stereo equipment
Verify DVD/disc players and radios are operational
Raise and lower roof mounted antenna if equipped
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Shower/Tub Enclosure
Visually inspect the glass panels, curtains and soap dish areas
Evaluate and rate the seals around the frame work and doors for water leaks
Operate the door and latch system to verify its operation
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Running Gear (Towables)
Type and number of axles
Inspect the frame, axles, springs, rims and other components for rust, oil stains and visible damage
Document the information on the tires as to their age and weight capacities
Check tire pressure
Inspect and rate tire tread condition
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Hitch System/Hook Up
Inspect and identify the type of system used to tow vehicle
 Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Leveling System
Operate by extending and retracting system
Check for hydraulic leaks or mechanic issues
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
CLASS A, B, C or Trailer with Generator

FLUID ANALSIS- Engine, Radiator and Transmission
Test for salt water intrusion, dirt and metal shavings

OBD Check for codes 

UNDERCARRIAGE
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
Bent frame or other
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
STEERING
Missing bolts nuts
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
  
DRIVE SHAFT
Bent
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
 
REAR END
Missing Nuts Bolts or bent
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
  
TRANSMISSION
Leaking…Case shows signs of Curb Damage
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
  
ENGINE
Oil Pan Leaking …signs of damage or repair
Yes…..No…..Not Present….SEE CERTIFIED TECHNICIAN
  
Weight Labels and Data Plates
Identify and document the Vehicle Identification Number (VIN)
Document the license plate info
List the inspection sticker information � if applicable
List the RVIA inspection seal number
List the Gross Vehicle Weight Rating
List date of manufacture
 



PARKEROCEANIC LLC
3555 John Bragg Hwy
Woodbury, TN 37190
parkeroceanic@yahoo.com
615-439-8820

3rd PARTY RV, SHIP or YACHT INSPECTION AGREEMENT TYPE
 
CIRCLE ONE BELOW
 
Bank Walkthrough - Basic – Essential – Plus - Premier
 
[bookmark: _Hlk15622763]This agreement is between CUSTOMER NAME: ________________________and ParkerOceanic LLC.
Customer home address.
Where you live (NOT where the RV or Owner is located NOT) ____________________________________________.

This is a New 3rd Party Agreement 'Inspection' between - CUSTOMER and ParkerOceanic  RV, SHIP or YACHT Inspections.

The Vehicle Identification Number (VIN) of the Vehicle is:
____________________________________________________________________________.

Brand, Model and Type of  Vehicle:
____________________________________________________________________________.

Street Address, State and Location where the  Vehicle Inspection is to take place:

Where the UNIT is physically located … where it will be at time of inspection?
 _____________________________________________________________.
 
Owners name and phone number____________________________________
 
Fee for the RV, SHIP or YACHT Inspection is $ _______ deposit is to be made to the account of ParkerOceanic LLC via PAY NOW BUTTON ON THIS PAGE AND HOME PAGE VIA SQUARE CREDIT CARD PROCESSING .........OR ZELLE using my ID email.... yacht1bnb@gmail.com ....phone number 209-420-3220......using my I.D. email …. parkeroceanic@yahoo.com. …. Dolan David Parker …. 615-439-8820.
 
Travel outside of the 50-mile radius of _________________ shall be 1.50 per mile for a total inspection and roundtrip travel cost of ________________.
ParkerOceanic LLC Inspections shall receive payment of $ _____________ from client before leaving for inspection. THIS AGREEMENT made this day ____________, year __________________, by and between ParkerOceanic LLC RV Inspections (hereinafter RV INSPECTOR) and the undersigned CUSTOMER collectively referred to herein as the parties. The Parties understand and voluntarily agree as follows:

1.  INSPECTOR AGREES TO MEET WITH CUSTOMER AT THE RV SITE.
 INSPECTOR agrees to perform a limited, non-invasive, visual inspection of the RV, SHIP or YACHT and to provide CLIENT with a written report identifying the defects that INSPECTOR both observed and deemed material.  INSPECTOR may offer comments as a courtesy, but these comments will not comprise the bargained-for report. The report is only supplementary to the sellers disclosure.
2. Unless otherwise inconsistent with this Agreement or not possible,  INSPECTOR agrees to perform the inspection in accordance with the US COAST GUARD Inspection Sheet CLIENT understands that US NAVY, US COAST GUARD nor the NRVIA is a party to this Agreement and has no control over INSPECTOR or representations made by  INSPECTOR and does not supervise  INSPECTOR. Unless otherwise indicated below, CLIENT understands that  INSPECTOR will NOT be testing for the presence of radon a colorless, odorless, radioactive gas that may be harmful to humans. CLIENT understands that  INSPECTOR will not test for compliance with applicable building codes or for the presence of potential dangers arising from asbestos, lead paint, formaldehyde, molds, contamination, and other environmental hazards or violations.
3. The inspection and report are for the use of CLIENT only.  INSPECTOR shall be the sole owner of the report and all rights to it.  INSPECTOR accepts no responsibility for use or misinterpretation by third parties, and third parties who rely on it in any way do so at their own risk and release  INSPECTOR (including employees and business entities) from any liability whatsoever. Any third parties who rely on the report in any way also agree to all provisions within this Agreement.  INSPECTORS inspection of the and the report are in no way a guarantee or warranty, express or implied, regarding the future use, operability, habitability or suitability of the  or its components. All warranties, express or implied, including warranties of merchantability and fitness for a particular purpose, are expressly excluded. CLIENT understands that structures have unique characteristics that make it impossible for the Inspector to inspect and evaluate them by an exterior visual inspection. Therefore, the scope of the inspection to be performed pursuant to this Agreement does not include any inspection of decay or hidden defects of the interior of the floor, walls, roofs, and other areas that are not accessible.
4.  INSPECTOR assumes no liability for the cost of repair or replacement of unreported defects or deficiencies either current or arising in the future. CLIENT acknowledges that the liability of  CONTRACT AGREEMENT SHOULD BE REVIEWED BY YOUR ATTORNEY BEFORE USE.
INSPECTOR, its agents and/or employees, for claims or damages, costs of defense or suit, attorneys fees and expenses arising out of or related to the  INSPECTORS negligence or breach of any obligation under this Agreement, including errors and omissions in the inspection or the report, shall be limited to liquidated damages in an amount equal to the fee paid to the INSPECTOR, and this liability shall be exclusive. CLIENT waives any claim for consequential, exemplary, special or incidental damages or for the loss of the use of even if the CLIENT has been advised of the possibility of such damages. The parties acknowledge that the liquidated damages are not intended as a penalty but are intended (i) to reflect the fact that actual damages may be difficult and impractical to ascertain; (ii) to allocate risk among the INSPECTOR and CLIENT; and (iii) to enable the INSPECTOR to perform the inspection at the stated fee.
5. INSPECTOR does not perform engineering, architectural, plumbing, or any other job function requiring an occupational license or certifications in the jurisdiction where the inspection is taking place. PARKER DOES NOT OWN NOR REPRESENT ANY OF THE FOLLOWING AGENCIES OR COMPANIES....US COAST GUARD, US NAVY, CUMMINS, DETROIT, FREIGHTLINER, LIPPERT, NRVIA, SKOOL, LEMON FINDER, HOMEGUAGE, EC LUBRICANTS NOR ANY OTHER ENTITY.
BUYER MUST HAVE ALL SYSTEMS RUNNING BEFORE INSPECTOR ARRIVES OR ITEM WILL BE MARKED INOPERABLE…NOT FUNTIONING AS DESIGNED. WE DO NOT REPAIR SYSYEMS LIKE WATER OR PROPANE AND TAKE NO RESPONSIBILITY FOR FROZEN PIPES OR GAS LEAKS.
6. In the event of a claim against INSPECTOR, CLIENT agrees to supply INSPECTOR with the following: (1) written notification of adverse conditions within 7 days of inspection completion; and (2) access to the vehicle. Failure to comply with the above conditions will release INSPECTOR and its agents from any and all obligations or liability of any kind.
7. Dispute Resolution; Binding Arbitration: Any dispute, controversy, interpretation or claim including claims for, but not limited to, breach of contract, any form of negligence, fraud or misrepresentation arising out of, from or related to this contract or arising out of, from or related to the inspection and inspection report shall be submitted for final and binding arbitration under the Rules and procedures of the American Arbitration Association. CLIENT agrees to pay all required filing fees. The decision of the Arbitrator appointed thereunder shall be final and binding and judgment on the Award may be entered in any course of competent jurisdiction.
8. If any provision of this Contract is held unenforceable, then such provision will be modified to reflect the parties intention. All remaining provisions of this Contract shall remain in full force and effect. This Agreement represents the entire agreement between the parties. All prior communications are merged into this Agreement, and there are no terms or conditions other than those set forth herein. No statement or promise of INSPECTOR or its agents shall be binding unless reduced to writing and signed by INSPECTOR. No change shall be enforceable against any party unless it is in writing and signed by the parties. This Agreement shall be binding upon and enforceable by the parties and their heirs, executors, administrators, successors and assignees. CLIENT shall have no cause of action against INSPECTOR after one year from the date of the inspection.
9. Payment of the fee to INSPECTOR is due prior to the start of the on-site recreational vehicle inspection. The CLIENT agrees to pay all legal and time expenses incurred in collecting due payments, including attorneys fees if any. If CLIENT is a corporation, LLC, or similar entity, the person signing this Agreement on behalf of such entity does personally guaranty payment of the fee by the entity.
10. If CLIENT requests a re-inspection, the re-inspection is also subject to all the terms and conditions set forth in this agreement.
11. This Agreement is not transferable or assignable.
12. Refunds are at the discretion of the Inspector and due within 30 days of written request for refund. Inspector reserves the right to transfer the inspection fee to a second chosen by customer.
13. The parties acknowledge that each of them has had ample opportunity for their own counsel to participate in negotiating and drafting this Agreement. Therefore, no rule of construction shall apply to this Agreement that construes ambiguous or unclear language in favor of or against any party.
CLIENT HAS CAREFULLY READ THE FOREGOING, AGREES TO IT, AND ACKNOWLEDGES RECEIPT OF A COPY OF THIS AGREEMENT.

FOR ParkerOceanic LLC YACHT-SHIP-RV Inspections
_______________________________________________________DATE:________________

CLIENT OR REPRESENTATIVE Signature* Printed Name
*One signature binds spouses/partners

_____________________________________________________DATE:_______________


